Model 5402 Dante Firmware

File Name: M5402v1r3r0.dnt

Version History:

Version: 1.3.0
Release Date: 28-Jul-2022
Description: Corrects error displaying Dante Secondary IP Address. Miscellaneous corrections and improvements. (Brooklyn II Firmware v4.2.7.4)
Technical Note: Dante Secondary Gateway Address may not display correctly.
Use Note: This is an engineering build from Audinate. It has not gone through their entire QC process. Studio Technologies feels that the improvements it contains warrants its release. (Caveat Emptor.)

Version: 1.2.0
Release Date: 16-Aug-2021
Description: Changes default Network Switch Configuration to Switched+Mgmt. Makes Enable Sync to External read only in Dante Controller. (Brooklyn II v4.2.3.13)
Firmware Use Note: Correct Model 5402 operation using this version requires that the unit also be using Main MCU Firmware version 1.01 or later and Main FPGA Firmware version 1.04 or later.
Technical Note: It's possible that the Dante secondary IP address will not display correctly on the Model 5402's front panel display and/or web interface pages. Audinate is aware of this issue and expects it will be corrected in the next release of the Brooklyn II firmware.

Version: 1.1.0
Release Date: 29-Jun-2021
Description: Adds support for 176.4 and 192 kHz sample rates. (Brooklyn II v4.2.0.28)
Firmware Use Note: Correct Model 5402 operation using this version requires that the unit also be using Main MCU Firmware version 1.01 or later and Main FPGA Firmware version 1.04 or later. 

Version: 1.0.0
Release Date: 08-Apr-2021
Description: Initial release. (Brooklyn II v4.2.0.28)
