Model M5412-01 Dante Firmware

File Name: M5412-01v4r4r0.dnt

Version History:

Version: 4.4.0
Release Date: 23-Aug-2022
Description: Corrects error displaying Dante Secondary IP Address. Miscellaneous corrections and improvements. (Brooklyn II Firmware v4.2.7.4)
Use Note: This is an engineering build from Audinate. It has not gone through their entire QC process. Studio Technologies feels that the improvements it contains warrants its release. (Caveat Emptor.)

Version: 4.3.0
Release Date: 27-Sep-2021
Description: Maintenance release which delivers a range of bug fixes. (Brooklyn II Firmware v4.2.3.13)
Technical Note: It's possible that the Dante secondary IP address will not display correctly on the Model 5412's front panel display and/or web interface pages. Audinate is aware of this issue and expects it will be corrected in the next release of the Brooklyn II firmware.

Version: 4.2.0
Release Date: 15-Aug-2019
Description: Adds support for SMPTE ST 2110-30 RTP audio transport for DDM enrolled devices. Adds support for AES67 RTP audio transport for DDM enrolled devices. Adds dynamic enable/disable of AES67 mode. Adds support for "wide flows"; Tx multicast flows can now be created with up to 64 channels. (Doesn't directly impact Model 5412-01.) Adds support for redundant RTP multicast flows. Includes many bug fixes and general improvements. (Brooklyn II Firmware v4.2.0.28)

Version: 4.1.1
Release Date: 24-May-2019
Description: Resolves known Precision Time Protocol (PTP), AES67, and subscription issues. (Brooklyn II Firmware v4.1.1.4)

Version: 1.1.0
Release Date: 29-Jan-2019
Description: Initial Release. (Brooklyn II v4.0.9.1)
