Model 5401 Dante Firmware

File Name: M5401v4r4r1.dnt

Version History:

Version: 4.4.1
Release Date: 26-Sep-2022
Description: Corrects error displaying Dante Secondary IP Address. Miscellaneous corrections and improvements. (Brooklyn II Firmware v4.2.7.4)
Use Note: This is an engineering build from Audinate. It has not gone through their entire QC process. Studio Technologies feels that the improvements it contains warrants its release. (Caveat Emptor.) 

Version: 4.3.0
Release Date: 27-Sep-2021
Description: Maintenance release which delivers a range of bug fixes. (Brooklyn II Firmware v4.2.3.13)

Version: 4.2.0
Release Date: 15-Aug-2019
Description: Adds support for SMPTE ST 2110-30 RTP audio transport for DDM enrolled devices. Adds support for AES67 RTP audio transport for DDM enrolled devices. Adds dynamic enable/disable of AES67 mode. Adds support for "wide flows"; Tx multicast flows can now be created with up to 64 channels. (Doesn't directly impact Model 5401.) Adds support for redundant RTP multicast flows. Includes many bug fixes and general improvements. (Brooklyn II Firmware v4.2.0.28)
Warning: Ensure that the Model 5401 is running Main Firmware version 1.04 or higher before loading this Dante Firmware version!

Version: 4.1.2
Release Date: 07-Aug-2019
Description: Corrects displayed Manufacturer Name. (Brooklyn II Firmware v4.1.1.4)
Warning: Ensure that the Model 5401 is running Main Firmware version 1.04 or higher before loading this Dante Firmware version!

Version: 4.1.1
Release Date: 24-May-2019
Description: Resolves known Precision Time Protocol (PTP), AES67, and subscription issues. (Brooklyn II Firmware v4.1.1.4)
Warning: Ensure that the Model 5401 is running Main Firmware version 1.04 or higher before loading this Dante Firmware version!

Version: 4.1.0
Release Date: 22-Feb-2018
Description: Resolves known Precision Time Protocol (PTP) issues. (Brooklyn II Firmware v4.0.8.2) 
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with the primary Ethernet connection unplugged.
Warning: Ensure that the Model 5401 is running Main Firmware version 1.04 or higher before loading this Dante Firmware version!

Version: 4.0.1
Release Date: 11-Dec-2017
Description: Adds additional factory diagnostic tools. (Brooklyn II v4.0.7.8)
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with the primary Ethernet connection unplugged.
Warning: Ensure that the Model 5401 is running Main Firmware version 1.04 or higher before loading this Dante Firmware version!

Version: 4.0.0
Release Date: 21-Nov-2017
Description: Adds support for Dante Domain Manager (DDM). Requires use of Model 5401 Application Firmware version 1.03 or later. (Brooklyn II v4.0.7.8) 
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with the primary Ethernet connection unplugged.
Warning: Ensure that the Model 5401 is running Main Firmware version 1.03 or higher before loading this Dante Firmware version!

Version: 1.1.0
Release Date: 19-Sep-2017
Description: Management Port now only available on Primary Network Connector in Redundant Network Configuration. Renamed Split Network Configuration "Pri Dante/Sec Mgmt". (Brooklyn II v3.10.2.2)
Warning: Ensure that the Model 5401 is running Main Firmware version 1.02 or higher before loading this Dante Firmware version!

Version: 1.0.0
Release Date: 30-Aug-2017
Description: Initial Release. (Brooklyn II v3.10.2.2)
