Model 5422-01 Dante Firmware

File Name: M5422-01v4r4r0.dnt

Version History:

Version: 4.4.0
Release Date: 26-Sep-2022
Description: Corrects error displaying Dante Secondary IP Address. Miscellaneous corrections and improvements. (Brooklyn II Firmware v4.2.7.4)
Use Note: This is an engineering build from Audinate. It has not gone through their entire QC process. Studio Technologies feels that the improvements it contains warrants its release. (Caveat Emptor.) 

Version: 4.3.0
Release Date: 27-Sep-2021
Description: Maintenance release which delivers a range of bug fixes. (Brooklyn II Firmware v4.2.3.13)

Version: 4.2.0
Release Date: 15-Aug-2019
Description: Adds support for SMPTE ST 2110-30 RTP audio transport for DDM enrolled devices. Adds support for AES67 RTP audio transport for DDM enrolled devices. Adds dynamic enable/disable of AES67 mode. Adds support for "wide flows"; Tx multicast flows can now be created with up to 64 channels. (Allows up to 32 channels for Model 5422-01.) Adds support for redundant RTP multicast flows. Includes many bug fixes and general improvements. (Brooklyn II Firmware v4.2.0.28)
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 4.1.2
Release Date: 07-Aug-2019
Description: Corrects displayed Manufacturer Name. (Brooklyn II Firmware v4.1.1.4)
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 4.1.1
Release Date: 24-May-2019
Description: Resolves known Precision Time Protocol (PTP), AES67, and subscription issues. (Brooklyn II Firmware v4.1.1.4)
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 4.1.0
Release Date: 22-Feb-2018
Description: Resolves known Precision Time Protocol (PTP) issues. (Brooklyn II Firmware v4.0.8.2)
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with the primary Ethernet connection unplugged.
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 4.0.1
Release Date: 11-Dec-2017
Description: Adds additional factory diagnostic tools. (Brooklyn II v4.0.7.8)
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with no Ethernet connection to primary network port.
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 4.0.0
Release Date: 05-Dec-2017
Description: Adds support for Dante Domain Manager (DDM). (Brooklyn II v4.0.7.8) 
Known Issue: Device will not pass audio if DDM is not present and unit is rebooted with no Ethernet connection to primary network port.
Warning: Ensure that the Model 5422-01 is running Main Firmware version 1.10 or higher before loading this Dante Firmware version!

Version: 1.1.0
Release Date: 10-Oct-2017
Description: In Redundant network configuration the management port is now only available via the primary network connector. Renamed "Split" network configuration to "Pri Dante/Sec Mgmt". No longer allows "Enable Sync To External" function to be enabled. (Brooklyn II v3.10.2.2)

Version: 1.0.3
Release Date: 06-Mar-2017
Description: Combines Capability and Brooklyn II Firmware into a single DNT file. (Brooklyn II v3.10.1.2)

Version: 1.0.2
Release Date: 09-Feb-2017
Description: Initial Release. (Brooklyn II v3.10.1.2)