Model 792 Dante Firmware

File Name: M792v4r3r0.dnt

Version History:

Version: 4.4.0
Release Date: 23-Aug-2022
Description: Corrects error displaying Dante Secondary IP Address. Miscellaneous corrections and improvements. (Brooklyn II Firmware v4.2.7.4)
Use Note: This is an engineering build from Audinate. It has not gone through their entire QC process. Studio Technologies feels that the improvements it contains warrants its release. (Caveat Emptor.)

Version: 4.3.0
Release Date: 27-Sep-2021
Description: Maintenance release which delivers a range of bug fixes. (Brooklyn II Firmware v4.2.3.13)

Version: 4.2.2
Release Date: 20-Nov-2020
Description: Updates Rx and Tx channel labels. (Brooklyn II Firmware v4.2.0.28)

Version: 4.2.1
Release Date: 25-Aug-2020
Description: Changes Model Name to Model 792 Central Controller. (Brooklyn II Firmware v4.2.0.28)

Version: 4.2.0
Release Date: 15-Aug-2019
Description: Adds support for SMPTE ST 2110-30 RTP audio transport for DDM enrolled devices. Adds support for AES67 RTP audio transport for DDM enrolled devices. Adds dynamic enable/disable of AES67 mode. Adds support for "wide flows"; Tx multicast flows can now be created with up to 64 channels. (Allows up to 16 channels for Model 792.) Adds support for redundant RTP multicast flows. Includes many bugs fixes and general improvements. (Brooklyn II Firmware v4.2.0.28)

Version: 4.1.2
Release Date: 07-Aug-2019
Description: Corrects displayed Manufacturer Name. (Brooklyn II Firmware v4.1.1.4)

Version: 4.1.1
Release Date: 24-May-2019
Description: Resolves known Precision Time Protocol (PTP), AES67, and subscription issues. (Brooklyn II Firmware v4.1.1.4)

Version: 1.0.0
Release Date: 19-Mar-2019
Description: Initial Release. (Brooklyn II Firmware v4.0.8.2)